

**Profiles**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Quantity | Type | Beam Angle | Wattage | Lamp | Frame Size (mm) | Weight | Irises | Gobo Holders |
| 6 | Sil Turbo | 11/26 | 1200 | T29 | 245x245 | 9.0kg |  |  |
| 8 | Source4 19deg | 19 | 750 | HPL750 | 160x160 | 7.0kg |  |  |
| 12 | Source4 26deg | 26 | 750 | HPL750 | 160x160 | 7.0kg |
| 6 | Source4 36deg | 36 | 750 | HPL750 | 160x160 | 7.0kg |
| 4 | Source4 50deg | 50 | 750 | HPL750 | 160x160 | 7.0kg |
| 12 | Source4 Junior | 25/50 | 575 | HPL575 | 160x160 | 8.5kg |  |  |
| 8 | Sil 30 | 22/40 | 1000 | T11 | 180x180 | 11.0kg |  |  |
| **Notes:** N/A | | | | | | | | |

**Fresnels/PCs**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Quantity | Type | Beam Angle | Wattage | Lamp | Frame Size (mm) | Weight | Barn Doors | Notes |
| 18 | Patt 743 | 15/82 | 1000 | T19/T11 | 210x210 | 9.2kg | 17 Doors |  |
| 13 | Berkey Colortran | 6/65 | 1000 | T19/T11 | 180x180 | 4.5kg | 13 Doors |  |
| 2 | Patt 243 | 16/50 | 2000 | CP43 | 290x290 | 14.0kg | 2 Doors |  |
| 10 | Minuette F | 18/57 | 500/650 | T18/T26 | 120x120 | 2.2kg |  |  |
| 4 | Minuette PC | 8/52 | 500/650 | T18/T26 | 120x120 | 2.8kg |  |
| **Notes:** N/A | | | | | | | | |

**PARs**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Quantity | Type | Beam Angle | Wattage | Lamp | Frame Size (mm) | Weight | Barn Doors | Notes |
| 46 | PAR 64 | - | 1000 | CP60/60/62 | 250x250 | 2.0kg | N/A |  |
| 6 | PAR 56 (Short Nose) | - | 500 | - | 225x225 | 1.7kg | N/A |  |
|  | PAR 16 (Birdie) 240V | - | 50/75 | GU10 type | 70x70 | 0.2kg | N/A |  |
|  | PAR 16 (Birdie) 12V |  | 50/75 | GU5.2 type | 70x70 | 0.2kg | N/A |  |
| **Notes:** N/A | | | | | | | | |

**Floods**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Quantity | Type | Beam Angle | Wattage | Lamp | Frame Size (mm) | Weight | Barn Doors | Notes |
| 4 | James Thomas 4 Cell Batten |  | 1000 | K4/K1 | 295x295 | 16.0kg | N/A |  |
| 4 | Strand Coda 4 Cell Batten |  | 500 | K1K9 | 235x215 | 4.5kg | N/A |  |
| 4 | Desisti Flood |  | 150 |  |  | 1.2kg | N/A |  |
| 2 | Light Technology UV Flood |  | 400 |  |  |  |  |  |
| **Notes:** N/A | | | | | | | | |

**Dimming**

* 118x 2.5KW Strand LD-90
* 12x 5.0KW Strand LD-90

**Control**

* ETC ION with fader wing. 1024 channels.

**Projection**

* CHRISTIE XL700 Projector
* 1x Standard Lens 1.8/2.4
* 1x Fixed Lens 0.8
* 2x DMX projector shutters

**Effects**

* 2x LOOK SOLUTIONS Unique 1.x Haze machines
* 1x LOOK SOLUTIONS Viper Smoke machine
* 1x Snow Machine

**Followspots**

* 2x ROBERT JULIATT Buxie 575W MSD